
-------------------
[version]
Signature="$Windows NT$"
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%Provider%
DriverVer=12/06/99
[Manufacturer]
%Provider%=Provider
[ControlFlags]
[Provider]
%CW10.DeviceDescPRISM2%= CW10.ndi, PCMCIA\D-Link_DWL-650_11Mbps_WLAN_Card-F360
[CW10.ndi]
[CW10.ndi.NT]
AddReg=Common.reg, Pcmcia.reg, nt.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=8
;CpyFiles=CW10.CopyFiles
[CW10_PCI.ndi.NT]
AddReg=Common.reg, PCI.reg, nt.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=8
;CpyFiles=CW10.CopyFiles
[CW10.ndi.NT.Services]
AddService=CW10, 2, CW10.Service, common.EventLog
[CW10_PCI.ndi.NT.Services]
AddService=CW10, 2, CW10.Service, common.EventLog
[DestinationDirs]
CW10.CopyFiles=12 ; system32\drivers subdirectory on NT
CW10.PCICopyFiles=12 ; system32\drivers subdirectory on NT
[CW10.CopyFiles]
cw10.sys,,,2 ; NT Installation
[SourceDiskNames]
1=%ROM_Description%,,,
[SourceDisksFiles]
[Common.reg]
HKR,,VendorDesc,0,"D-Link DWL-650 11Mbps WLAN Adapter"
HKR,,APDensity,,1
HKR,defaults,APDensity,,1
HKR,,SSID,,%SSID_DEF_STR%
HKR,defaults,SSID,,%SSID_DEF_STR%
HKR,NDI\params\SSID,ParamDesc,,"SSID"
HKR,NDI\params\SSID,type,,edit
HKR,NDI\params\SSID,limitText,,32
HKR,NDI\params\SSID,default,,%SSID_DEF_STR%
HKR,NDI\params\SSID,flag,1,30,00,00,00
HKR,,StationName,,"Client"
HKR,defaults,StationName,,"Client"
HKR,,LAA,,""
HKR,,ListenInterval,0,3
HKR,defaults,ListenInterval,0,3
HKR,NDI\params\ListenInterval,,0,3
HKR,NDI\params\ListenInterval,ParamDesc,,"Maximum Listen Interval"
HKR,NDI\params\ListenInterval,flag,1,30,00,00,00
HKR,NDI\params\ListenInterval,type,,int
HKR,Ndi\params\ListenInterval,default,,3
HKR,NDI\params\ListenInterval,min,0,0
HKR,NDI\params\ListenInterval,max,0,77
HKR,NDI\params\ListenInterval,step,0,1
HKR,NDI\params\ListenInterval,optional,0,0
HKR,,DSChannel,,6
HKR,defaults,DSChannel,,6
HKR,NDI\params\Channel,ParamDesc,,"Channel"
HKR,NDI\params\Channel,type,,enum
HKR,NDI\params\Channel,default,,6
HKR,NDI\params\Channel,flag,1,20,00,00,00
HKR,NDI\params\Channel\enum,1,,"Channel 1"
HKR,NDI\params\Channel\enum,2,,"Channel 2"
HKR,NDI\params\Channel\enum,3,,"Channel 3"
HKR,NDI\params\Channel\enum,4,,"Channel 4"
HKR,NDI\params\Channel\enum,5,,"Channel 5"
HKR,NDI\params\Channel\enum,6,,"Channel 6"
HKR,NDI\params\Channel\enum,7,,"Channel 7"
HKR,NDI\params\Channel\enum,8,,"Channel 8"
HKR,NDI\params\Channel\enum,9,,"Channel 9"
HKR,NDI\params\Channel\enum,10,,"Channel 10"
HKR,NDI\params\Channel\enum,11,,"Channel 11"
HKR,NDI\params\Channel\enum,12,,"Channel 12"
HKR,NDI\params\Channel\enum,13,,"Channel 13"
HKR,NDI\params\Channel\enum,14,,"Channel 14"
HKR,,Encapsulation,,1
HKR,defaults,Encapsulation,,1
HKR, ,TxRate, ,15
HKR, defaults,TxRate, ,15
HKR, NDI\params\TxRate, ParamDesc, , "Transmit Rate"
HKR, NDI\params\TxRate, type, , enum
HKR, NDI\params\TxRate, default, , 15
HKR, NDI\params\TxRate,flag, 1, 30, 00, 00, 00
HKR, NDI\params\TxRate\enum, 1, ,"Fixed 1 Mb/s"
HKR, NDI\params\TxRate\enum, 2, ,"Fixed 2 Mb/s"
HKR, NDI\params\TxRate\enum, 3, ,"Auto Select 1 or 2"
HKR, NDI\params\TxRate\enum, 4, ,"Fixed 5.5 Mb/s"
HKR, NDI\params\TxRate\enum, 8, ,"Fixed 11 Mb/s"
HKR, NDI\params\TxRate\enum, 15, ,"Fully Auto"
HKR, ,RTSThresh, 0, 2432
HKR, defaults,RTSThresh, 0, 2432
HKR, NDI\params\RTSThresh, ParamDesc, , "Medium Reservation"
HKR, NDI\params\RTSThresh, type, , enum
HKR, NDI\params\RTSThresh, default, , 2432
HKR, NDI\params\RTSThresh, flag, 1, 30, 00, 00, 00
HKR, NDI\params\RTSThresh\enum, 2432, , "Off"
HKR, NDI\params\RTSThresh\enum, 500, , "Hidden Stations"
HKR, ,FragThresh, 0, 2432
HKR, defaults,FragThresh, 0, 2432
HKR, NDI\params\FragThresh, ,0, 2432
HKR, NDI\params\FragThresh, ParamDesc, 0,"Fragmentation Threshold"
HKR, NDI\params\FragThresh, type, 0,int
HKR, Ndi\params\FragThresh, default, 0,2432
HKR, NDI\params\FragThresh, min, 0,256
HKR, NDI\params\FragThresh, max, 0,2432
HKR, NDI\params\FragThresh, step, 0,128
HKR, NDI\params\FragThresh, flag, 1,20,00,00,00
HKR, NDI\params\FragThresh, optional, 0,0
HKR,,NetworkType,,%NETWORK_TYPE_DEF_STR%
HKR,defaults,NetworkType,,%NETWORK_TYPE_DEF_STR%
HKR,NDI\params\NetworkType,ParamDesc,,"Network Type"
HKR,NDI\params\NetworkType,type,,enum
HKR,NDI\params\NetworkType,default,,%NETWORK_TYPE_DEF_STR%
HKR,NDI\params\NetworkType,flag,1,30,00,00,00
HKR,NDI\params\NetworkType\enum,0,,"802.11 Ad Hoc"
HKR,NDI\params\NetworkType\enum,1,,"Infrastructure"
HKR,NDI\params\NetworkType\enum,3,,"Ad Hoc"
HKR,,PSMode,,1
HKR,defaults,PSMode,,1
HKR,NDI\params\PSMode,ParamDesc,,"Power Save Mode"
HKR,NDI\params\PSMode,type,,enum
HKR,NDI\params\PSMode,default,,1
HKR,NDI\params\PSMode,flag,1,30,00,00,00
HKR,NDI\params\PSMode\enum,1,,"Disabled"
HKR,NDI\params\PSMode\enum,2,,"Enabled"
HKR,,WepReq,0,0
HKR,defaults,WepReq,0,0
HKR,NDI\params\WepReq,,0,0
HKR,NDI\params\WepReq,ParamDesc,,"Encryption"
HKR,NDI\params\WepReq,flag,1,30,00,00,00
HKR,NDI\params\WepReq,type,,enum
HKR,Ndi\params\WepReq,default,,0
HKR,NDI\params\WepReq\enum,0,,"Disabled"
HKR,NDI\params\WepReq\enum,2,,"64 bit"
HKR,NDI\params\WepReq\enum,6,,"128 bit"
HKR,NDI\params\WepReq,optional,0,0
HKR,,EncryptInDriver,0,1
HKR,defaults,EncryptInDriver,0,1
HKR,,DecryptInDriver,0,1
HKR,defaults,DecryptInDriver,0,1
HKR,,WEPFactor,0,3
HKR,defaults,WEPFactor,0,3
HKR,,PreambleMode,0,1
HKR,defaults,PreambleMode,0,1
HKR,NDI\params\PreambleMode,,0,1
HKR,NDI\params\PreambleMode,ParamDesc,,%SHORT_PREAM_STR%
HKR,NDI\params\PreambleMode,flag,1,30,00,00,00
HKR,NDI\params\PreambleMode,type,,enum
HKR,Ndi\params\PreambleMode,default,,1
HKR,NDI\params\PreambleMode\enum,1,,"Long Tx Preamble"
HKR,NDI\params\PreambleMode\enum,2,,"Short Tx Preamble"
HKR,NDI\params\PreambleMode\enum,3,,"Auto"
HKR,NDI\params\PreambleMode,optional,0,0
HKR,,AuthentAlg,,%AUTHENT_TYPE_DEF_STR%
HKR,defaults,AuthentAlg,,%AUTHENT_TYPE_DEF_STR%
HKR,NDI\params\AuthentAlg,ParamDesc,,"Authentication Algorithm"
HKR,NDI\params\AuthentAlg,type,,enum
HKR,NDI\params\AuthentAlg,default,,%AUTHENT_TYPE_DEF_STR%
HKR,NDI\params\AuthentAlg,flag,1,30,00,00,00
HKR,NDI\params\AuthentAlg\enum,1,,"WECA Compliant (always use Open)"
HKR,NDI\params\AuthentAlg\enum,2,,"Must use Shared with WEP"
HKR,,Esarhpssap,,"dlink"
HKR,defaults,Esarhpssap,,"dlink"
HKR,NDI\params\Esarhpssap,ParamDesc,,"WEP Passphrase"
HKR,NDI\params\Esarhpssap,type,,edit
HKR,NDI\params\Esarhpssap,limitText,,64
HKR,NDI\params\Esarhpssap,default,,"dlink"
HKR,NDI\params\Esarhpssap,flag,1,30,00,00,00
HKR,,IBSSInDriver,0,1
HKR,defaults,IBSSInDriver,0,1
HKR,NDI\params\IBSSInDriver,,0,1
HKR,NDI\params\IBSSInDriver,ParamDesc,,"Driver based IBSS"
HKR,NDI\params\IBSSInDriver,type,,enum
HKR,NDI\params\IBSSInDriver,default,,1
HKR,NDI\params\IBSSInDriver,flag,1,30,00,00,00
HKR,NDI\params\IBSSInDriver\enum,0,,"Disabled"
HKR,NDI\params\IBSSInDriver\enum,1,,"Enabled"
[Pcmcia.reg]
HKR,,PollInDriver,0,0
HKR,defaults,PollInDriver,0,0
HKR,NDI\params\PollInDriver,,0,0
HKR,NDI\params\PollInDriver,ParamDesc,,"Driver Polling"
HKR,NDI\params\PollInDriver,type,,enum
HKR,NDI\params\PollInDriver,default,,0
HKR,NDI\params\PollInDriver,flag,1,30,00,00,00
HKR,NDI\params\PollInDriver\enum,0,,"Disabled"
HKR,NDI\params\PollInDriver\enum,1,,"Enabled"
[PCI.reg]
HKR,,PollInDriver,0,1
HKR,defaults,PollInDriver,0,1
HKR,NDI\params\PollInDriver,,0,1
HKR,NDI\params\PollInDriver,ParamDesc,,"Driver Polling"
HKR,NDI\params\PollInDriver,type,,enum
HKR,NDI\params\PollInDriver,default,,1
HKR,NDI\params\PollInDriver,flag,1,30,00,00,00
HKR,NDI\params\PollInDriver\enum,0,,"Disabled"
HKR,NDI\params\PollInDriver\enum,1,,"Enabled"
[nt.reg]
HKR, , BusType, 0, "8" ; PCMCIA
HKR, Ndi, Service, 0, "CW10"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis4"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
[CW10.Service]
DisplayName=%CW10.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_AUTO_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\CW10.sys
LoadOrderGroup=NDIS
[common.EventLog]
AddReg=common.AddEventLog.reg
[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000,"%%SystemRoot%%\System32\netevent.dll,%%SystemRoot%%\System32\drivers\CW10.sys"
HKR, , TypesSupported, 0x00010001, 7
[Strings]
Provider="D-Link Corporation"
CW10="CW10"
CW10.DeviceDescPRISM2="D-Link DWL-650 11Mbps WLAN Adapter"
CW10.Service.DispName="Prism Wireless LAN Win2K Driver"
SHORT_PREAM_STR ="Preamble Mode"
SSID_DEF_STR="default"
NETWORK_TYPE_DEF_STR="1"
AUTHENT_TYPE_DEF_STR="2"
ROM_Description=""
