
[Version]
DriverVer=01/12/2004, 1.0.8.0
Signature="$Chicago$"
Compatible=1
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%VER_VENDOR_STR%
CatalogFile=WUSB54G.cat
[ControlFlags]
ExcludeFromSelect=*
[Manufacturer]
%VER_VENDOR_NAME_STR%=DeviceList
[DeviceList]
%WUSB54G%=USB20_PID2234, USB\VID_1915&PID_2234
%WUSB54GP%=USB20_PID2235, USB\VID_1915&PID_2235
%WUSB54G%=USB20_G, USB\VID_5041&PID_2234
%WUSB54GP%=USB20_GP, USB\VID_5041&PID_2235
[USB20_PID2234]
AddReg=USB20_PID2234.reg, COMMON_A02.reg, COMMON_NDIS.reg, COMMON.reg
;CpyFiles=USB_DRIVER.copy
[USB20_PID2234.NT]
AddReg=USB20_PID2234.reg, COMMON_A02.reg, COMMON_NDIS.reg.NT, COMMON.reg
;CpyFiles=USB_DRIVER.copy.NT
BusType=15
Characteristics= 0x84
[USB20_PID2235]
AddReg=USB20_PID2235.reg, COMMON_A02.reg, COMMON_NDIS.reg, COMMON.reg
;CpyFiles=USB_DRIVER.copy
[USB20_PID2235.NT]
AddReg=USB20_PID2235.reg, COMMON_A02.reg, COMMON_NDIS.reg.NT, COMMON.reg
;CpyFiles=USB_DRIVER.copy.NT
BusType=15
Characteristics= 0x84
[USB20_G]
AddReg=USB20_G.reg, COMMON_A02.reg, COMMON_NDIS.reg, COMMON.reg
;CpyFiles=USB_DRIVER.copy
[USB20_G.NT]
AddReg=USB20_G.reg, COMMON_A02.reg, COMMON_NDIS.reg.NT, COMMON.reg
;CpyFiles=USB_DRIVER.copy.NT
BusType=15
Characteristics= 0x84
[USB20_GP]
AddReg=USB20_GP.reg, COMMON_A02.reg, COMMON_NDIS.reg, COMMON.reg
;CpyFiles=USB_DRIVER.copy
[USB20_GP.NT]
AddReg=USB20_GP.reg, COMMON_A02.reg, COMMON_NDIS.reg.NT, COMMON.reg
;CpyFiles=USB_DRIVER.copy.NT
BusType=15
Characteristics= 0x84
[USB20_PID2234.NT.Services]
AddService= "PRISM_A02", 2, PRISM_DRIVER_A02.Service, PRISM_DRIVER.EventLog
[USB20_PID2235.NT.Services]
AddService= "PRISM_A02", 2, PRISM_DRIVER_A02.Service, PRISM_DRIVER.EventLog
[USB20_G.NT.Services]
AddService= "PRISM_A02", 2, PRISM_DRIVER_A02.Service, PRISM_DRIVER.EventLog
[USB20_GP.NT.Services]
AddService= "PRISM_A02", 2, PRISM_DRIVER_A02.Service, PRISM_DRIVER.EventLog
[USB20_PID2234.reg]
HKR,Ndi,DeviceID,0,"USB\VID_1915&PID_2234"
HKR,,PlatformID,0,14480
HKR,,VendorDesc,0,%WUSB54G%
[USB20_PID2235.reg]
HKR,Ndi,DeviceID,0,"USB\VID_1915&PID_2235"
HKR,,PlatformID,0,14480
HKR,,VendorDesc,0,%WUSB54GP%
[USB20_G.reg]
HKR,Ndi,DeviceID,0,"USB\VID_5041&PID_2234"
HKR,,PlatformID,0,14480
HKR,,VendorDesc,0,%WUSB54G%
[USB20_GP.reg]
HKR,Ndi,DeviceID,0,"USB\VID_5041&PID_2235"
HKR,,PlatformID,0,14480
HKR,,VendorDesc,0,%WUSB54GP%
[PRISM_DRIVER_A02.Service]
DisplayName=%WUSB54GSRV%
ServiceType=1 ; SERVICE_KERNEL_DRIVER
StartType=3 ; SERVICE_DEMAND_START
ErrorControl=1 ; NORMAL
ServiceBinary=%12%\WUSB20XP.sys
LoadOrderGroup=NDIS
[PRISM_DRIVER.EventLog]
AddReg=PRISM_DRIVER.EventLog.reg
[PRISM_DRIVER.EventLog.reg]
HKR, ,EventMessageFile ,0x00020000 ,"%%SystemRoot%%\System32\netevent.dll"
HKR, ,TypesSupported ,0x00010001 ,7
[COMMON_A02.reg]
HKR,NDI ,Service ,0 ,"PRISM_A02"
HKR,NDI ,CardType ,0 ,"USB"
HKR, ,BusType ,0 ,"0"
[COMMON_NDIS.reg]
HKR, ,DeviceVxDs ,0 ,"WUSB209x.sys"
HKR, ,RunningWin9X ,0 ,"1"
HKR, ,DevLoader ,0 ,"*ndis"
HKR, ,EnumPropPages ,0 ,"netdi.dll,EnumPropPages"
HKR,NDI\Interfaces ,UpperRange ,0 ,"ndis3"
HKR,NDI\Interfaces ,LowerRange ,0 ,"ethernet"
HKR,NDI\Interfaces ,DefUpper ,0 ,"ndis3"
HKR,NDI\Interfaces ,DefLower ,0 ,"ethernet"
HKR,NDIS ,LogDriverName ,0 ,"WUSB209x"
HKR,NDIS ,MajorNdisVersion ,1 ,03
HKR,NDIS ,MinorNdisVersion ,1 ,0a
[COMMON_NDIS.reg.NT]
HKR,NDI\Interfaces ,UpperRange ,0 ,"ndis5"
HKR,NDI\Interfaces ,LowerRange ,0 ,"ethernet"
[COMMON.reg]
HKR, ,PRISMIOC ,0 ,"1"
HKR, ,SilentInstall ,0 ,"1"
HKR,,RTSThresh,0,2432
HKR,Ndi\params\RTSThresh,default,0,2347
HKR,NDI\params\RTSThresh,ParamDesc,0,%RTSTHRESH_STR%
HKR,NDI\params\RTSThresh,type,0,int
HKR,NDI\params\RTSThresh,flag,1,20,00,00,00
HKR,NDI\params\RTSThresh,min,0,0
HKR,NDI\params\RTSThresh,max,0,2347
HKR,NDI\params\RTSThresh,step,0,1
HKR,NDI\params\RTSThresh,optional,0,1
HKR,,FragThresh,0,2346
HKR,Ndi\params\FragThresh,default,0,2346
HKR,NDI\params\FragThresh,ParamDesc,0,%FRAGTHRESH_STR%
HKR,NDI\params\FragThresh,type,0,int
HKR,NDI\params\FragThresh,flag,1,20,00,00,00
HKR,NDI\params\FragThresh,min,0,256
HKR,NDI\params\FragThresh,max,0,2346
HKR,NDI\params\FragThresh,step,0,2
HKR,NDI\params\FragThresh,optional,0,1
HKR,,ShortRetryLimit,0,7
HKR,NDI\params\ShortRetryLimit,default,0,7
HKR,NDI\params\ShortRetryLimit,ParamDesc,,%SHORT_RETRY_STR%
HKR,NDI\params\ShortRetryLimit,type,,int
HKR,NDI\params\ShortRetryLimit,min,0,1
HKR,NDI\params\ShortRetryLimit,max,0,255
HKR,NDI\params\ShortRetryLimit,step,0,1
HKR,NDI\params\ShortRetryLimit,optional,0,1
HKR,,LongRetryLimit,0,4
HKR,NDI\params\LongRetryLimit,default,0,4
HKR,NDI\params\LongRetryLimit,ParamDesc,,%LONG_RETRY_STR%
HKR,NDI\params\LongRetryLimit,type,0,int
HKR,NDI\params\LongRetryLimit,min,0,1
HKR,NDI\params\LongRetryLimit,max,0,255
HKR,NDI\params\LongRetryLimit,step,0,1
HKR,NDI\params\LongRetryLimit,optional,0,1
HKR,,ConfigProfile,0,256
HKR,NDI\params\ConfigProfile,default,0,256
HKR,NDI\params\ConfigProfile,ParamDesc,,%CONFIG_PROFILE%
HKR,NDI\params\ConfigProfile,type,,enum
HKR,NDI\params\ConfigProfile,flag,1,30,00,00,00
HKR,NDI\params\ConfigProfile\enum,0,,%CONFIG_PROF_B_ONLY%
HKR,NDI\params\ConfigProfile\enum,1,,%CONFIG_PROF_MIXED%
HKR,NDI\params\ConfigProfile\enum,2,,%CONFIG_PROF_MIXED_LONG%
HKR,NDI\params\ConfigProfile\enum,3,,%CONFIG_PROF_G_ONLY%
HKR,NDI\params\ConfigProfile\enum,5,,%CONFIG_PROF_B_WIFI%
HKR,NDI\params\ConfigProfile\enum,6,,%CONFIG_PROF_MIXED_SHORT%
HKR,NDI\params\ConfigProfile\enum,256,,%CONFIG_PROF_WIFI_SPEC%
HKR,NDI\params\ConfigProfile,optional,0,1
HKR,,NitroMode,0,"1"
HKR,,PSMode,0,1
HKR,Ndi\params\PSMode,default,0,1
HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
HKR,NDI\params\PSMode,type,,enum
HKR,NDI\params\PSMode,flag,1,30,00,00,00
HKR,NDI\params\PSMode\enum,1,,%POWER_SAVE_OFF_STR%
HKR,NDI\params\PSMode\enum,2,,%POWER_SAVE_DYN_STR%
HKR,NDI\params\PSMode\enum,3,,%POWER_SAVE_MAX_STR%
HKR,NDI\params\PSMode,optional,0,1
[DestinationDirs]
DefaultDestDir=11
USB_DRIVER.copy=11
USB_DRIVER.copy.NT=12
[USB_DRIVER.copy]
WUSB209x.sys
[USB_DRIVER.copy.NT]
WUSB20XP.sys
[SourceDisksNames]
1=%INSTALL_DISK_STR%,,,
[SourceDisksFiles]
WUSB209x.sys=1
[SourceDisksFiles.X86]
WUSB20XP.sys=1
[Strings]
VER_VENDOR_STR="The Cisco-Linksys, LLC."
VER_VENDOR_NAME_STR="The Cisco-Linksys, LLC."
WUSB54G="Linksys Wireless-G USB Network Adapter"
WUSB54GP="Linksys Wireless-G Portable USB Adapter"
WUSB54GSRV="802.11a/g USB Driver"
INSTALL_DISK_STR="Linksys Wireless-G USB Network Adapter Install Disk"
ON_STR="On"
OFF_STR="Off"
RTSTHRESH_STR="RTS Threshold"
FRAGTHRESH_STR="Fragmentation Threshold"
AUTHENT_TYPE_STR="Authentication Algorithm"
POWER_SAVE_STR="Power Save Mode"
POWER_SAVE_OFF_STR="Disabled"
POWER_SAVE_DYN_STR="Dynamic"
POWER_SAVE_MAX_STR="Maximum"
SHORT_RETRY_STR="Short Retry Limit"
LONG_RETRY_STR="Long Retry Limit"
CONFIG_PROFILE="Configuration Profile"
CONFIG_PROF_B_ONLY="B only"
CONFIG_PROF_MIXED="Mixed"
CONFIG_PROF_MIXED_LONG="Mixed Long"
CONFIG_PROF_G_ONLY="G only"
CONFIG_PROF_TEST="Test"
CONFIG_PROF_B_WIFI="B WiFi"
CONFIG_PROF_MIXED_SHORT="Mixed Short"
CONFIG_PROF_WIFI_SPEC="WiFi Spec"
NITRO_MODE="Nitro Mode"
