
[version]
Signature="$Windows NT$" ; Combined Win9x/Win2k inf
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%V_BCM%
Compatible=1
DriverVer=02/09/2005, 3.100.46.5
CatalogFile=USRMAXG.CAT
[Manufacturer]
%V_BCM%=BROADCOM,NTx86.5.1
[ControlFlags]
ExcludeFromSelect=*
[BROADCOM.ntx86.5.1]
%BCM430G_DeviceDesc%=BCM43XG, PCI\VEN_14E4&DEV_4318&SUBSYS_011916EC&REV_02
%BCM430PCI_DeviceDesc%=BCM43XG, PCI\VEN_14E4&DEV_4318&SUBSYS_011A16EC&REV_02
[BROADCOM]
%BCM430G_DeviceDesc%=BCM43XG, PCI\VEN_14E4&DEV_4318&SUBSYS_011916EC&REV_02
%BCM430PCI_DeviceDesc%=BCM43XG, PCI\VEN_14E4&DEV_4318&SUBSYS_011A16EC&REV_02
[BCM43XG]
AddReg=BCM43XX.win.reg, BCM43XX.win.brcm.reg, common.reg, g.options.reg, bg.options.reg
DelReg=common.delreg, rate.delreg
;CpyFiles=BCM43XX.sys.files
DriverVer=02/09/2005, 3.100.46.5
[BCM43XX.win.reg]
HKR, Ndi, DeviceID, , "PCI\VEN_14E4&DEV_4307"
HKR, , EnumPropPages, 0, "netdi.dll,EnumPropPages"
HKR, NDIS, MajorNdisVersion, 1, 03
HKR, NDIS, MinorNdisVersion, 1, 0A
HKR, NDIS, LogDriverName, , "BCM43XX"
HKR, NDIS, MajorDriverVersion, 1, 1
HKR, NDIS, MinorDriverVersion, 1, 0
HKR, Ndi\Install, , , "BCM43XX.ndi.install"
HKR, Ndi\Interfaces, DefUpper, 0, "ndis3"
HKR, Ndi\Interfaces, DefLower, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis3"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
[BCM43XX.win.brcm.reg]
HKR, Ndi, HelpText, , %BCM43XX_HELP%
[BCM43XX.ndi.install]
AddReg=BCM43XX.ndi.reg
[BCM43XX.ndi.reg]
HKR, , DevLoader, 0, "*ndis"
HKR, , DeviceVxDs, 0, "BCMWL5.SYS"
[BCM43XX.sys.files]
BCMWL5.SYS,,,2
[BCM43XG.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX.reg, BCM43XX.brcm.reg, common.reg, g.options.reg, bg.options.reg
DelReg=common.delreg, rate.delreg
;CpyFiles=BCM43XX.files.NT
DriverVer=02/09/2005, 3.100.46.5
[BCM43XG.NT.Services]
AddService=BCM43XX, 2, BCM43XX.Service, common.EventLog
[BCM43XX.reg]
HKR, Ndi\Interfaces, UpperRange, , "ndis5"
HKR, Ndi\Interfaces, LowerRange, , "ethernet"
[BCM43XX.brcm.reg]
HKR, Ndi, HelpText, , %BCM43XX_HELP%
HKR, Ndi, Service, 0, "BCM43XX"
[BCM43XX.Service]
DisplayName=%BCM43XX_Service_DispName%
ServiceType=1 ; %SERVICE_KERNEL_DRIVER%
StartType=3 ; %SERVICE_DEMAND_START%
ErrorControl=1 ; %SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\bcmwl5.sys
LoadOrderGroup=NDIS
[common.EventLog]
AddReg=common.AddEventLog.reg
[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported, 0x00010001, 7
[BCM43XX.files.NT]
BCMWL5.SYS,,,2
[common.delreg]
HKR, Ndi\params\RoamPref
HKR, Ndi\params\AssocPref
HKR, Ndi\params\Locale
HKR,,Locale
[rate.delreg]
HKR, Ndi\params\Rate
HKR, Ndi\params\RateA
[common.reg]
HKR, ,"EnableSoftAP", 0, "0"
HKR, ,"EnableAutoConnect", 0, "0"
HKR, Ndi\params\Country, ParamDesc, 0, %Location%
HKR, Ndi\params\Country, type, 0, "enum"
HKR, Ndi\params\Country\enum, "", 0, %Default%
HKR, Ndi\params\Country, default,, ""
HKR, Ndi\params\RoamDelta, ParamDesc, 0, %RoamingTendency%
HKR, Ndi\params\RoamDelta, type, 0, "enum"
HKR, Ndi\params\RoamDelta\enum, "0", 0, %Aggressive%
HKR, Ndi\params\RoamDelta\enum, "1", 0, %Moderate%
HKR, Ndi\params\RoamDelta\enum, "2", 0, %Conservative%
HKR, Ndi\params\RoamDelta,default,,"1"
HKR, Ndi\params\RadioState, ParamDesc, 0, %RadioEnableDisable%
HKR, Ndi\params\RadioState, type, 0, "enum"
HKR, Ndi\params\RadioState\enum, "1", 0, %Disabled%
HKR, Ndi\params\RadioState\enum, "0", 0, %Enabled%
HKR, Ndi\params\RadioState,default,,"0"
HKR, Ndi\params\MPC, ParamDesc, 0, %MiminumPowerConsumption%
HKR, Ndi\params\MPC, type, 0, "enum"
HKR, Ndi\params\MPC\enum, "0", 0, %Disabled%
HKR, Ndi\params\MPC\enum, "1", 0, %Enabled%
HKR, Ndi\params\MPC,default,,"1"
HKR, Ndi\params\PowerSaveMode, ParamDesc, 0, %PowerSaveMode%
HKR, Ndi\params\PowerSaveMode, type, 0, "enum"
HKR, Ndi\params\PowerSaveMode\enum, "0", 0, %Disabled%
HKR, Ndi\params\PowerSaveMode\enum, "1", 0, %Enabled%
HKR, Ndi\params\PowerSaveMode\enum, "2", 0, %Fast%
HKR, Ndi\params\PowerSaveMode,default,,"0"
HKR, Ndi\params\frag, ParamDesc, 0, %FragmentationThreshold%
HKR, Ndi\params\frag,type,0,"dword"
HKR, Ndi\params\frag,min,,"256"
HKR, Ndi\params\frag,max,,"2346"
HKR, Ndi\params\frag,default,,"2346"
HKR, Ndi\params\rts, ParamDesc, 0, %RTSThreshold%
HKR, Ndi\params\rts,type,0,"dword"
HKR, Ndi\params\rts,min,,"0"
HKR, Ndi\params\rts,max,,"2347"
HKR, Ndi\params\rts,default,,"2347"
HKR, Ndi\params\NetworkAddress, ParamDesc, 0, %LocallyAdministeredMACAddress%
HKR, Ndi\params\NetworkAddress, type, 0, "edit"
HKR, Ndi\params\NetworkAddress, LimitText, 0, "12"
HKR, Ndi\params\NetworkAddress, UpperCase, 0, "1"
HKR, Ndi\params\NetworkAddress, default, 0, ""
HKR, Ndi\params\NetworkAddress, optional, 0, "1"
HKR, Ndi\params\PwrOut, ParamDesc, 0, %PowerOutput%
HKR, Ndi\params\PwrOut, type, 0, "enum"
HKR, Ndi\params\PwrOut\enum, "100", 0, "100%"
HKR, Ndi\params\PwrOut\enum, "75", 0, "75%"
HKR, Ndi\params\PwrOut\enum, "50", 0, "50%"
HKR, Ndi\params\PwrOut\enum, "25", 0, "25%"
HKR, Ndi\params\PwrOut,default,,"100"
HKR, Ndi\params\FrameBursting, ParamDesc, 0, %XPress_Technology%
HKR, Ndi\params\FrameBursting, type, 0, "enum"
HKR, Ndi\params\FrameBursting\enum, "0", 0, %Disabled%
HKR, Ndi\params\FrameBursting\enum, "1", 0, %Enabled%
HKR, Ndi\params\FrameBursting,default,,"1"
HKR, Ndi\params\BTCoexist, ParamDesc, 0, %BlueToothCollaboration%
HKR, Ndi\params\BTCoexist, type, 0, "enum"
HKR, Ndi\params\BTCoexist\enum, "1", 0, %Enable%
HKR, Ndi\params\BTCoexist\enum, "0", 0, %Disable%
HKR, Ndi\params\BTCoexist,default,,"0"
HKR,,"WEP",0, ""
HKR,,"NetworkType", 0, "-1"
HKR,,"SSID", 0, ""
HKR,,"gpio0", 0, "-1"
HKR,,"gpio1", 0, "-1"
HKR,,"gpio2", 0, "-1"
HKR,,"gpio3", 0, "-1"
HKR,,"scan_channel_time", 0,"-1"
HKR,,"scan_unassoc_time", 0,"-1"
HKR,,"scan_home_time", 0,"-1"
HKR,,"scan_passes", 0,"-1"
HKR,,"BadFramePreempt", 0,"0"
HKR,,"Interference_Mode", 0,"3"
HKR,,"ccx_rm", 0,"1"
HKR,,"ccx_rm_limit", 0,"300"
HKR, Ndi\params\antdiv, ParamDesc, 0, %AntennaDiversity%
HKR, Ndi\params\antdiv, type, 0, "enum"
HKR, Ndi\params\antdiv\enum, "-1", 0, %Auto%
HKR, Ndi\params\antdiv,default,,"-1"
HKR, Ndi\params\WME, ParamDesc, 0, %WME%
HKR, Ndi\params\WME, type, 0, "enum"
HKR, Ndi\params\WME\enum, "1", 0, %Enabled%
HKR, Ndi\params\WME\enum, "0", 0, %Disabled%
HKR, Ndi\params\WME,default,,"0"
HKLM, Software\Broadcom\802.11, PerUserPN, 0x00010001, 0
HKLM, Software\Broadcom\802.11, DisallowPNChanges, 0x00010001, 0
HKR, Ndi\params\WZCCoexist, ParamDesc,0, %WZC_Managed_Ethernet%
HKR, Ndi\params\WZCCoexist, type, 0, "enum"
HKR, Ndi\params\WZCCoexist\enum, "0", 0, %Disabled%
HKR, Ndi\params\WZCCoexist\enum, "1", 0, %Enabled%
HKR, Ndi\params\WZCCoexist,default,,"0"
HKR, Ndi\params\IBSSLink, ParamDesc, 0, %IBSS_Link_Indication%
HKR, Ndi\params\IBSSLink, type, 0, "enum"
HKR, Ndi\params\IBSSLink\enum, "0", 0, %Legacy%
HKR, Ndi\params\IBSSLink\enum, "1", 0, %Default%
HKR, Ndi\params\IBSSLink,default,,"1"
[b.options.reg]
HKR, Ndi\params\PLCPHeader, ParamDesc, 0, %PLCPHeader%
HKR, Ndi\params\PLCPHeader, type, 0, "enum"
HKR, Ndi\params\PLCPHeader\enum, "-1", 0, %Long%
HKR, Ndi\params\PLCPHeader\enum, "0", 0, %AutoShortLong%
HKR, Ndi\params\PLCPHeader,default,,"0"
HKR, Ndi\params\Rate, ParamDesc, 0, %Rate%
HKR, Ndi\params\Rate, type, 0, "enum"
HKR, Ndi\params\Rate\enum, "0", 0, %Usebestrate%
HKR, Ndi\params\Rate\enum, "2", 0, " 1"
HKR, Ndi\params\Rate\enum, "4", 0, " 2"
HKR, Ndi\params\Rate\enum, "11", 0, " 5.5"
HKR, Ndi\params\Rate\enum, "22", 0, "11"
HKR, Ndi\params\Rate,default,,"0"
[g.options.reg]
HKR, Ndi\params\RoamTrigger, ParamDesc, 0, %RoamingDecision%
HKR, Ndi\params\RoamTrigger, type, 0, "enum"
HKR, Ndi\params\RoamTrigger\enum, "-60", 0, %OptimizeBandwidth%
HKR, Ndi\params\RoamTrigger\enum, "-70", 0, %Default%
HKR, Ndi\params\RoamTrigger\enum, "-80", 0, %OptimizeDistance%
HKR, Ndi\params\RoamTrigger,default,,"-70"
HKR, Ndi\params\PLCPHeader, ParamDesc, 0, %BSSPLCPHeader%
HKR, Ndi\params\PLCPHeader, type, 0, "enum"
HKR, Ndi\params\PLCPHeader\enum, "-1", 0, %Long%
HKR, Ndi\params\PLCPHeader\enum, "0", 0, %AutoShortLong%
HKR, Ndi\params\PLCPHeader,default,,"0"
HKR, Ndi\params\IBSSGMode, ParamDesc, 0, %IBSS54gtmMode%
HKR, Ndi\params\IBSSGMode, type, 0, "enum"
HKR, Ndi\params\IBSSGMode\enum, "0", 0, %80211bOnly%
HKR, Ndi\params\IBSSGMode\enum, "1", 0, %54gLRS%
HKR, Ndi\params\IBSSGMode\enum, "2", 0, %54gAuto%
HKR, Ndi\params\IBSSGMode\enum, "4", 0, %54gPerformance%
HKR, Ndi\params\IBSSGMode,default,,"2"
HKR, Ndi\params\IBSSGProtection, ParamDesc, 0, %IBSS54gtmProtectionMode%
HKR, Ndi\params\IBSSGProtection, type, 0, "enum"
HKR, Ndi\params\IBSSGProtection\enum, "0", 0, %Disabled%
HKR, Ndi\params\IBSSGProtection\enum, "2", 0, %Auto%
HKR, Ndi\params\IBSSGProtection,default,,"2"
HKR, Ndi\params\Rate, ParamDesc, 0, %Rate%
HKR, Ndi\params\Rate, type, 0, "enum"
HKR, Ndi\params\Rate\enum, "0", 0, %Usebestrate%
HKR, Ndi\params\Rate\enum, "2", 0, " 1"
HKR, Ndi\params\Rate\enum, "4", 0, " 2"
HKR, Ndi\params\Rate\enum, "11", 0, " 5.5"
HKR, Ndi\params\Rate\enum, "12", 0, " 6"
HKR, Ndi\params\Rate\enum, "18", 0, " 9"
HKR, Ndi\params\Rate\enum, "22", 0, "11"
HKR, Ndi\params\Rate\enum, "24", 0, "12"
HKR, Ndi\params\Rate\enum, "36", 0, "18"
HKR, Ndi\params\Rate\enum, "48", 0, "24"
HKR, Ndi\params\Rate\enum, "72", 0, "36"
HKR, Ndi\params\Rate\enum, "96", 0, "48"
HKR, Ndi\params\Rate\enum, "108", 0, "54"
HKR, Ndi\params\Rate,default,,"0"
HKR, Ndi\params\Afterburner, ParamDesc, 0, %Afterburner%
HKR, Ndi\params\Afterburner, type, 0, "enum"
HKR, Ndi\params\Afterburner\enum, "0", 0, %Disabled%
HKR, Ndi\params\Afterburner\enum, "1", 0, %Enabled%
HKR, Ndi\params\Afterburner,default,,"1"
[bg.options.reg]
HKR, Ndi\params\Channel, ParamDesc, 0, %IBSSChannelNumber%
HKR, Ndi\params\Channel, default, 0, "11"
HKR, Ndi\params\Channel, min, 0, "1"
HKR, Ndi\params\Channel, max, 0, "14"
HKR, Ndi\params\Channel, step, 0, "1"
HKR, Ndi\params\Channel, base, 0, "10"
HKR, Ndi\params\Channel, type, 0, "int"
HKR, Ndi\params\ApCompatMode, ParamDesc, 0, %ApCompatibilityMode%
HKR, Ndi\params\ApCompatMode, type, 0, "enum"
HKR, Ndi\params\ApCompatMode\enum, "1", 0, %BroaderCompat%
HKR, Ndi\params\ApCompatMode\enum, "0", 0, %HigherPerf%
HKR, Ndi\params\ApCompatMode,default,,"0"
[a.options.reg]
HKR, Ndi\params\Afterburner, ParamDesc, 0, %Afterburner%
HKR, Ndi\params\Afterburner, type, 0, "enum"
HKR, Ndi\params\Afterburner\enum, "0", 0, %Disabled%
HKR, Ndi\params\Afterburner\enum, "1", 0, %Enabled%
HKR, Ndi\params\Afterburner,default,,"1"
HKR, Ndi\params\RateA, ParamDesc, 0, %Rate_802_11a%
HKR, Ndi\params\RateA, type, 0, "enum"
HKR, Ndi\params\RateA\enum, "0", 0, %Usebestrate%
HKR, Ndi\params\RateA\enum, "12", 0, " 6"
HKR, Ndi\params\RateA\enum, "18", 0, " 9"
HKR, Ndi\params\RateA\enum, "24", 0, "12"
HKR, Ndi\params\RateA\enum, "36", 0, "18"
HKR, Ndi\params\RateA\enum, "48", 0, "24"
HKR, Ndi\params\RateA\enum, "72", 0, "36"
HKR, Ndi\params\RateA\enum, "96", 0, "48"
HKR, Ndi\params\RateA\enum, "108",0, "54"
HKR, Ndi\params\RateA,default,,"0"
HKR, Ndi\params\Channel, ParamDesc, 0, %IBSSChannelNumber%
HKR, Ndi\params\Channel, type, 0, "enum"
HKR, Ndi\params\Channel\enum, "36", 0, " 36"
HKR, Ndi\params\Channel\enum, "40", 0, " 40"
HKR, Ndi\params\Channel\enum, "44", 0, " 44"
HKR, Ndi\params\Channel\enum, "48", 0, " 48"
HKR, Ndi\params\Channel\enum, "52", 0, " 52"
HKR, Ndi\params\Channel\enum, "56", 0, " 56"
HKR, Ndi\params\Channel\enum, "60", 0, " 60"
HKR, Ndi\params\Channel\enum, "64", 0, " 64"
HKR, Ndi\params\Channel\enum, "100", 0, "100"
HKR, Ndi\params\Channel\enum, "104", 0, "104"
HKR, Ndi\params\Channel\enum, "108", 0, "108"
HKR, Ndi\params\Channel\enum, "112", 0, "112"
HKR, Ndi\params\Channel\enum, "116", 0, "116"
HKR, Ndi\params\Channel\enum, "120", 0, "120"
HKR, Ndi\params\Channel\enum, "124", 0, "124"
HKR, Ndi\params\Channel\enum, "128", 0, "128"
HKR, Ndi\params\Channel\enum, "132", 0, "132"
HKR, Ndi\params\Channel\enum, "136", 0, "136"
HKR, Ndi\params\Channel\enum, "140", 0, "140"
HKR, Ndi\params\Channel, default, 0, "36"
[bag.options.reg]
HKR, Ndi\params\Afterburner, ParamDesc, 0, %Afterburner%
HKR, Ndi\params\Afterburner, type, 0, "enum"
HKR, Ndi\params\Afterburner\enum, "0", 0, %Disabled%
HKR, Ndi\params\Afterburner\enum, "1", 0, %Enabled%
HKR, Ndi\params\Afterburner,default,,"1"
HKR, Ndi\params\11HNetworks, ParamDesc, 0, "802.11h"
HKR, Ndi\params\11HNetworks, type, 0, "enum"
HKR, Ndi\params\11HNetworks\enum, "0", 0, %Disabled%
HKR, Ndi\params\11HNetworks\enum, "1", 0, %Loose%
HKR, Ndi\params\11HNetworks\enum, "2", 0, %Strict%
HKR, Ndi\params\11HNetworks,default,,"0"
HKR, Ndi\params\RoamTrigger, ParamDesc, 0, %RoamingDecision%
HKR, Ndi\params\RoamTrigger, type, 0, "enum"
HKR, Ndi\params\RoamTrigger\enum, "-60", 0, %OptimizeBandwidth%
HKR, Ndi\params\RoamTrigger\enum, "-70", 0, %Default%
HKR, Ndi\params\RoamTrigger\enum, "-80", 0, %OptimizeDistance%
HKR, Ndi\params\RoamTrigger,default,,"-70"
HKR, Ndi\params\PLCPHeader, ParamDesc, 0, %BSSPLCPHeader%
HKR, Ndi\params\PLCPHeader, type, 0, "enum"
HKR, Ndi\params\PLCPHeader\enum, "-1", 0, %Long%
HKR, Ndi\params\PLCPHeader\enum, "0", 0, %AutoShortLong%
HKR, Ndi\params\PLCPHeader,default,,"0"
HKR, Ndi\params\band, ParamDesc, 0, %DisableBands%
HKR, Ndi\params\band, type, 0, "enum"
HKR, Ndi\params\band\enum, "0", 0, %None%
HKR, Ndi\params\band\enum, "1", 0, %Disable80211gb%
HKR, Ndi\params\band\enum, "2", 0, %Disable80211a%
HKR, Ndi\params\band,default,,"0"
HKR, Ndi\params\BandPref, ParamDesc, 0, %BandPreference%
HKR, Ndi\params\BandPref, type, 0, "enum"
HKR, Ndi\params\BandPref\enum, "0", 0, %None%
HKR, Ndi\params\BandPref\enum, "1", 0, %Prefer80211a%
HKR, Ndi\params\BandPref\enum, "2", 0, %Prefer80211gb%
HKR, Ndi\params\BandPref,default,,"0"
HKR, Ndi\params\AssocRoamPref, ParamDesc, 0, %AssociationRoamPreference%
HKR, Ndi\params\AssocRoamPref, type, 0, "enum"
HKR, Ndi\params\AssocRoamPref\enum, "0", 0, %Disabled%
HKR, Ndi\params\AssocRoamPref\enum, "1", 0, %Enabled%
HKR, Ndi\params\AssocRoamPref,default,,"0"
HKR, Ndi\params\IBSSGMode, ParamDesc, 0, %IBSS54gtmMode%
HKR, Ndi\params\IBSSGMode, type, 0, "enum"
HKR, Ndi\params\IBSSGMode\enum, "0", 0, %80211bOnly%
HKR, Ndi\params\IBSSGMode\enum, "1", 0, %54gLRS%
HKR, Ndi\params\IBSSGMode\enum, "2", 0, %54gAuto%
HKR, Ndi\params\IBSSGMode\enum, "4", 0, %54gPerformance%
HKR, Ndi\params\IBSSGMode,default,,"2"
HKR, Ndi\params\IBSSGProtection, ParamDesc, 0, %IBSS54gtmProtectionMode%
HKR, Ndi\params\IBSSGProtection, type, 0, "enum"
HKR, Ndi\params\IBSSGProtection\enum, "0", 0, %Disabled%
HKR, Ndi\params\IBSSGProtection\enum, "2", 0, %Auto%
HKR, Ndi\params\IBSSGProtection,default,,"2"
HKR, Ndi\params\RateA, ParamDesc, 0, %Rate_802_11a%
HKR, Ndi\params\RateA, type, 0, "enum"
HKR, Ndi\params\RateA\enum, "0", 0, %Usebestrate%
HKR, Ndi\params\RateA\enum, "12", 0, " 6"
HKR, Ndi\params\RateA\enum, "18", 0, " 9"
HKR, Ndi\params\RateA\enum, "24", 0, "12"
HKR, Ndi\params\RateA\enum, "36", 0, "18"
HKR, Ndi\params\RateA\enum, "48", 0, "24"
HKR, Ndi\params\RateA\enum, "72", 0, "36"
HKR, Ndi\params\RateA\enum, "96", 0, "48"
HKR, Ndi\params\RateA\enum, "108", 0, "54"
HKR, Ndi\params\RateA,default,,"0"
HKR, Ndi\params\Rate, ParamDesc, 0, %Rate_802_11bg%
HKR, Ndi\params\Rate, type, 0, "enum"
HKR, Ndi\params\Rate\enum, "0", 0, %Usebestrate%
HKR, Ndi\params\Rate\enum, "2", 0, " 1"
HKR, Ndi\params\Rate\enum, "4", 0, " 2"
HKR, Ndi\params\Rate\enum, "11", 0, " 5.5"
HKR, Ndi\params\Rate\enum, "12", 0, " 6"
HKR, Ndi\params\Rate\enum, "18", 0, " 9"
HKR, Ndi\params\Rate\enum, "22", 0, "11"
HKR, Ndi\params\Rate\enum, "24", 0, "12"
HKR, Ndi\params\Rate\enum, "36", 0, "18"
HKR, Ndi\params\Rate\enum, "48", 0, "24"
HKR, Ndi\params\Rate\enum, "72", 0, "36"
HKR, Ndi\params\Rate\enum, "96", 0, "48"
HKR, Ndi\params\Rate\enum, "108", 0, "54"
HKR, Ndi\params\Rate,default,,"0"
HKR, Ndi\params\Channel, ParamDesc, 0, %IBSSChannelNumber%
HKR, Ndi\params\Channel, type, 0, "enum"
HKR, Ndi\params\Channel\enum, "1", 0, " 1"
HKR, Ndi\params\Channel\enum, "2", 0, " 2"
HKR, Ndi\params\Channel\enum, "3", 0, " 3"
HKR, Ndi\params\Channel\enum, "4", 0, " 4"
HKR, Ndi\params\Channel\enum, "5", 0, " 5"
HKR, Ndi\params\Channel\enum, "6", 0, " 6"
HKR, Ndi\params\Channel\enum, "7", 0, " 7"
HKR, Ndi\params\Channel\enum, "8", 0, " 8"
HKR, Ndi\params\Channel\enum, "9", 0, " 9"
HKR, Ndi\params\Channel\enum, "10", 0, " 10"
HKR, Ndi\params\Channel\enum, "11", 0, " 11"
HKR, Ndi\params\Channel\enum, "12", 0, " 12"
HKR, Ndi\params\Channel\enum, "13", 0, " 13"
HKR, Ndi\params\Channel\enum, "14", 0, " 14"
HKR, Ndi\params\Channel\enum, "36", 0, " 36"
HKR, Ndi\params\Channel\enum, "40", 0, " 40"
HKR, Ndi\params\Channel\enum, "44", 0, " 44"
HKR, Ndi\params\Channel\enum, "48", 0, " 48"
HKR, Ndi\params\Channel\enum, "52", 0, " 52"
HKR, Ndi\params\Channel\enum, "56", 0, " 56"
HKR, Ndi\params\Channel\enum, "60", 0, " 60"
HKR, Ndi\params\Channel\enum, "64", 0, " 64"
HKR, Ndi\params\Channel\enum, "100", 0, "100"
HKR, Ndi\params\Channel\enum, "104", 0, "104"
HKR, Ndi\params\Channel\enum, "108", 0, "108"
HKR, Ndi\params\Channel\enum, "112", 0, "112"
HKR, Ndi\params\Channel\enum, "116", 0, "116"
HKR, Ndi\params\Channel\enum, "120", 0, "120"
HKR, Ndi\params\Channel\enum, "124", 0, "124"
HKR, Ndi\params\Channel\enum, "128", 0, "128"
HKR, Ndi\params\Channel\enum, "132", 0, "132"
HKR, Ndi\params\Channel\enum, "136", 0, "136"
HKR, Ndi\params\Channel\enum, "140", 0, "140"
HKR, Ndi\params\Channel, default, 0, "11"
HKR, Ndi\params\ApCompatMode, ParamDesc, 0, %ApCompatibilityMode%
HKR, Ndi\params\ApCompatMode, type, 0, "enum"
HKR, Ndi\params\ApCompatMode\enum, "1", 0, %BroaderCompat%
HKR, Ndi\params\ApCompatMode\enum, "0", 0, %HigherPerf%
HKR, Ndi\params\ApCompatMode,default,,"0"
[DestinationDirs]
DefaultDestDir=11
BCM43XX.sys.files=11
BCM43XX.files.NT=12
[SourceDisksNames]
1=%BCM43XX_DiskName%,,
[SourceDisksFiles]
BCMWL5.SYS=1
[strings]
V_BCM="U.S. Robotics Corporation"
BCM430G_DeviceDesc="U.S. Robotics Wireless MAXg PC Card"
BCM430PCI_DeviceDesc="U.S. Robotics Wireless MAXg PCI Adapter"
BCM43XX_HELP="U.S. Robotics Wireless MAXg Adapter provides wireless local area networking."
BCM43XX_Service_DispName="U.S. Robotics Wireless MAXg Adapter"
BCM43XX_DiskName="U.S. Robotics Wireless MAXg Network Adapter Install Disk"
UnitedStates="United States"
54gAuto="54g - Auto"
54gLRS="54g - LRS"
54gPerformance="54g - Performance"
80211bOnly="802.11b Only"
AntennaDiversity="Antenna Diversity"
Auto="Auto"
AutoShortLong="Auto (Short/Long)"
BSSPLCPHeader="BSS PLCP Header"
BlueToothCollaboration="Bluetooth Collaboration"
Default="Default"
Disable="Disable"
Disable80211a="Disable 802.11a"
Disable80211gb="Disable 802.11g/b"
DisableBands="Disable Bands"
Disabled="Disabled"
Enable="Enable"
Enabled="Enabled"
FragmentationThreshold="Fragmentation Threshold"
IBSS54gtmMode="IBSS 54g Mode"
IBSS54gtmProtectionMode="IBSS 54g Protection Mode"
IBSSChannelNumber="IBSS Channel Number"
LocallyAdministeredMACAddress="Locally Administered MAC Address"
Long="Long"
None="None"
OptimizeBandwidth="Optimize Bandwidth"
OptimizeDistance="Optimize Distance"
PLCPHeader="PLCP Header"
PowerOutput="Power Output"
PowerSaveMode="Power Save Mode"
Prefer80211a="Prefer 802.11a"
Prefer80211gb="Prefer 802.11g/b"
RTSThreshold="RTS Threshold"
RadioEnableDisable="Radio Enable/Disable"
Rate="Rate"
RoamingDecision="Roaming Decision"
Usebestrate="Use best rate"
XPress_Technology="54g+ (XPress)"
Location="Location"
Strict="Strict"
Loose="Loose"
Fast="Fast"
MiminumPowerConsumption="Minimum Power Consumption"
AssociationRoamPreference="Association Roam Preference"
BandPreference="Band Preference"
RoamingTendency="Roam Tendency"
Aggressive="Aggressive"
Moderate="Moderate"
Conservative="Conservative"
ApCompatibilityMode="AP Compatibility Mode"
BroaderCompat="Broader Compatibility"
HigherPerf="Higher Performance"
WME="WME"
Afterburner="MAXg (125 Mbps)"
Rate_802_11a="Rate (802.11a)"
Rate_802_11bg="Rate (802.11b/g)"
WZC_Managed_Ethernet="WZC Managed Ethernet"
Legacy="Legacy"
IBSS_Link_Indication="IBSS Link Indication"

