
[Version]
Signature="$Windows NT$"
Compatible=1
Class=Net
ClassGUID={4D36E972-E325-11CE-BFC1-08002BE10318}
Provider=%MRVL%
CatalogFile=netmw125.cat
DriverVer=12/30/2005,3.2.3.2
[SourceDisksNames]
1="Marvell installation disk 1",,,
[SourceDisksFiles]
Mrvw123.sys=1
Mrvw125.sys=1
[DestinationDirs]
W8335PCI.XP.CopyFiles=12
W8335PCI.2K.CopyFiles=12
DefaultDestDirs=11
[Manufacturer]
%MRVL%=Marvell,NT.5.1
[Marvell]
%W8335PCI.DeviceDesc%=W8335PCI.ndi.NT, PCI\VEN_11AB&DEV_1FAA
%W8335PCI.DeviceDesc%=W8335PCI.ndi.NT, PCI\VEN_11AB&DEV_1FAA&SUBSYS_54011148
%W8335PXPCI.DeviceDesc%=W8335PCI.ndi.NT, PCI\VEN_11AB&DEV_1FAB
[Marvell.NT.5.1]
%W8335PCI.DeviceDesc%=W8335PCIXP.ndi, PCI\VEN_11AB&DEV_1FAA
%W8335PCI.DeviceDesc%=W8335PCIXP.ndi, PCI\VEN_11AB&DEV_1FAA&SUBSYS_54011148
%W8335PXPCI.DeviceDesc%=W8335PCIXP.ndi, PCI\VEN_11AB&DEV_1FAB
[ControlFlags]
ExcludeFromSelect=*
[W8335PCIXP.ndi]
Characteristics=0x84
BusType=5
AddReg=W8335PCI.reg, W8335PCIXP.reg, W8335PCIXP.zerocfg
;CpyFiles=W8335PCI.XP.CopyFiles
[W8335PCIXP.ndi.Services]
AddService=W8335XP, 2, W8335PCIXP.Service, CommonXP.EventLog
[W8335PCIXP.reg]
HKR, Ndi, Service, 0, "W8335XP"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
[W8335PCI.XP.CopyFiles]
Mrvw125.sys,,,2
[W8335PCIXP.Service]
DisplayName=%W8335PCIXP.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_DEMAND_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\Mrvw125.sys
LoadOrderGroup=NDIS
[CommonXP.EventLog]
AddReg=CommonXP.AddEventLog.reg
[CommonXP.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported, 0x00010001, 7
[W8335PCI.ndi.NT]
Characteristics=0x84
BusType=5
AddReg=W8335PCI.reg, W8335PCI2K.reg, W8335PCI.devID.reg
;CpyFiles=W8335PCI.2K.CopyFiles
DeviceID="PCI\VEN_11AB&DEV_1FAA"
[W8335PCI.ndi.NT.Services]
AddService=W8335PCI, 2, W8335PCI2K.Service, Common.EventLog
[W8335PCI2K.reg]
HKR, Ndi, Service, 0, "W8335PCI"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
[W8335PCI.2K.CopyFiles]
Mrvw123.sys,,,2
[W8335PCI2K.Service]
DisplayName=%W8335PCI2K.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_DEMAND_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\Mrvw123.sys
LoadOrderGroup=NDIS
[Common.EventLog]
AddReg=Common.AddEventLog.reg
[Common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported, 0x00010001, 7
[W8335PCI.devID.reg]
HKR, Ndi, DeviceID, 0, "PCI\VEN_11AB&DEV_1FAA"
[W8335PCI.reg]
HKR, Ndi\params\FragThsd, ParamDesc,0 , "%FragThsd%"
HKR, Ndi\params\FragThsd, default, 0 , "2346"
HKR, Ndi\params\FragThsd, min, 0 , "256"
HKR, Ndi\params\FragThsd, max, 0 , "2346"
HKR, Ndi\params\FragThsd, step, 0 , "1"
HKR, Ndi\params\FragThsd, Base, 0 , "10"
HKR, Ndi\params\FragThsd, type, 0 ,"dword"
HKR, Ndi\params\RTSThsd, ParamDesc, 0, "%RTSThsd%"
HKR, Ndi\params\RTSThsd, default, 0, "2346"
HKR, Ndi\params\RTSThsd, min, 0, "0"
HKR, Ndi\params\RTSThsd, max, 0, "2346"
HKR, Ndi\params\RTSThsd, step, 0, "1"
HKR, Ndi\params\RTSThsd, Base, 0, "10"
HKR, Ndi\params\RTSThsd, type, 0, "dword"
HKR, Ndi\params\PowerMode,ParamDesc,,"%PowerMode%"
HKR, Ndi\params\PowerMode,default,,"0"
HKR, Ndi\params\PowerMode,type,,enum
HKR, Ndi\params\PowerMode\enum,"0",,"CAM-Constantly Awake Mode"
HKR, Ndi\params\PowerMode\enum,"1",,"MaxPSP-Max Power Savings"
HKR, Ndi\params\ChannelRange,ParamDesc,,"%RegionControl%"
HKR, Ndi\params\ChannelRange,default,,"0"
HKR, Ndi\params\ChannelRange,type,,enum
HKR, Ndi\params\ChannelRange\enum,"0",,"Default"
HKR, Ndi\params\ChannelRange\enum,"010B",,"FCC"
HKR, Ndi\params\ChannelRange\enum,"010B",,"IC"
HKR, Ndi\params\ChannelRange\enum,"010D",,"ETSI"
HKR, Ndi\params\ChannelRange\enum,"0A0B",,"Spain"
HKR, Ndi\params\ChannelRange\enum,"0A0D",,"France"
HKR, Ndi\params\ChannelRange\enum,"0E0E",,"MKK"
HKR, Ndi\params\ChannelRange\enum,"010E",,"MKK1"
HKR, Ndi\params\ChannelRange\enum,"0309",,"Israel"
HKR, Ndi\params\Preamble,ParamDesc,,"%PreambleStr%"
HKR, Ndi\params\Preamble,default,,"3"
HKR, Ndi\params\Preamble,type,,enum
HKR, Ndi\params\Preamble\enum,"1",,"Auto"
HKR, Ndi\params\Preamble\enum,"2",,"Short Preamble"
HKR, Ndi\params\Preamble\enum,"3",,"Long Preamble"
HKR, Ndi\params\AdhocGMode,ParamDesc,,"%AdhocGMode%"
HKR, Ndi\params\AdhocGMode,default,,"1"
HKR, Ndi\params\AdhocGMode,type,,enum
HKR, Ndi\params\AdhocGMode\enum,"0",,"Adhoc G Mode"
HKR, Ndi\params\AdhocGMode\enum,"1",,"Adhoc B Mode only"
HKR, Ndi\params\DesiredSSID,ParamDesc,,"%SSID%"
HKR, Ndi\params\DesiredSSID,default,,"MarvellAP3x"
HKR, Ndi\params\DesiredSSID,type,,"edit"
HKR, Ndi\params\DesiredSSID,LimitText,,"32"
HKR, Ndi\params\DesiredSSID,UpperCase,,"0"
HKR, Ndi\params\DesiredSSID,Optional,,"0"
HKR, Ndi\params\WMM,ParamDesc,,"%WMM%"
HKR, Ndi\params\WMM,default,,"0"
HKR, Ndi\params\WMM,type,,enum
HKR, Ndi\params\WMM\enum,"0",,"Disable"
HKR, Ndi\params\WMM\enum,"1",,"Enable"
HKR, Ndi\xparams\WIFI,ParamDesc,,"%WIFI%"
HKR, Ndi\xparams\WIFI,default,,"0"
HKR, Ndi\xparams\WIFI,type,,enum
HKR, Ndi\xparams\WIFI\enum,"0",,"Disable"
HKR, Ndi\xparams\WIFI\enum,"1",,"Enable"
HKR, Ndi\xparams\AuthMode,ParamDesc,,"%AuthMode%"
HKR, Ndi\xparams\AuthMode,default,,"0"
HKR, Ndi\xparams\AuthMode,type,,enum
HKR, Ndi\xparams\AuthMode\enum,"0",,"Open"
HKR, Ndi\xparams\AuthMode\enum,"1",,"Shared"
HKR, Ndi\xparams\NetworkMode,ParamDesc,,"%NetworkMode%"
HKR, Ndi\xparams\NetworkMode,default,,"1"
HKR, Ndi\xparams\NetworkMode,type,,enum
HKR, Ndi\xparams\NetworkMode\enum,"0",,"Ad Hoc"
HKR, Ndi\xparams\NetworkMode\enum,"1",,"Infrastructure"
HKR, Ndi\params\Channel, ParamDesc,0 , "%Channel%"
HKR, Ndi\params\Channel, default, 0 , "1"
HKR, Ndi\params\Channel, min, 0 , "0"
HKR, Ndi\params\Channel, max, 0 , "14"
HKR, Ndi\params\Channel, step, 0 , "1"
HKR, Ndi\params\Channel, Base, 0 , "10"
HKR, Ndi\params\Channel, type, 0 ,"dword"
HKR, Ndi\xparams\TxAntenna, ParamDesc,0 , "%TxAntennaStr%"
HKR, Ndi\xparams\TxAntenna, default, 0 , "2"
HKR, Ndi\xparams\TxAntenna, min, 0 , "1"
HKR, Ndi\xparams\TxAntenna, max, 0 , "ffff"
HKR, Ndi\xparams\TxAntenna, step, 0 , "1"
HKR, Ndi\xparams\TxAntenna, Base, 0 , "16"
HKR, Ndi\xparams\TxAntenna, type, 0 ,"dword"
HKR, Ndi\xparams\RxAntenna, ParamDesc,0 , "%RxAntennaStr%"
HKR, Ndi\xparams\RxAntenna, default, 0 , "ffff"
HKR, Ndi\xparams\RxAntenna, min, 0 , "1"
HKR, Ndi\xparams\RxAntenna, max, 0 , "ffff"
HKR, Ndi\xparams\RxAntenna, step, 0 , "1"
HKR, Ndi\xparams\RxAntenna, Base, 0 , "16"
HKR, Ndi\xparams\RxAntenna, type, 0 ,"dword"
HKR,, LED0PowerOn, 2,"30001"
HKR,, LED1PowerOn, 2,"fe0101"
HKR,, LED0PowerOff, 2,"fe0000"
HKR,, LED1PowerOff, 2,"fe0100"
HKR,, LED0Scan, 2,"ff0002"
HKR,, LED1Scan, 2,"40102"
HKR,, LED0Associated, 2,"ff0005"
HKR,, LED1Associated, 2,"fe0105"
HKR,, LED0Joined, 2,"ff0006"
HKR,, LED1Joined, 2,"fe0106"
HKR,, LED0Started, 2,"30007"
HKR,, LED1Started, 2,"fe0107"
HKR,, LED0Tx, 2,"ff0008"
HKR,, LED1Tx, 2,"30108"
HKR,, LED0Rx, 2,"ff0009"
HKR,, LED1Rx, 2,"30109"
HKR,, LED0TxHigh, 2,"ff000c"
HKR,, LED1TxHigh, 2,"2010c"
HKR,, LED0RxHigh, 2,"ff000d"
HKR,, LED1RxHigh, 2,"2010d"
HKR, Ndi\xparams\LED0PowerOn,ParamDesc,,"%LED0PowerOnStr%"
HKR, Ndi\xparams\LED0PowerOn,default,,"ff0001"
HKR, Ndi\xparams\LED0PowerOn,type,,enum
HKR, Ndi\xparams\LED0PowerOn\enum,"ff0001",,"LED Stays On"
HKR, Ndi\xparams\LED0PowerOn\enum,"fe0001",,"LED Stays Off"
HKR, Ndi\xparams\LED0PowerOn\enum,"fd0001",,"No Change"
HKR, Ndi\xparams\LED0PowerOn\enum,"40001",,"Slow blink"
HKR, Ndi\xparams\LED0PowerOn\enum,"30001",,"Regular blink"
HKR, Ndi\xparams\LED0PowerOn\enum,"20001",,"Fast blink"
HKR, Ndi\xparams\LED1PowerOn,ParamDesc,,"%LED1PowerOnStr%"
HKR, Ndi\xparams\LED1PowerOn,default,,"fe0101"
HKR, Ndi\xparams\LED1PowerOn,type,,enum
HKR, Ndi\xparams\LED1PowerOn\enum,"ff0101",,"LED Stays On"
HKR, Ndi\xparams\LED1PowerOn\enum,"fe0101",,"LED Stays Off"
HKR, Ndi\xparams\LED1PowerOn\enum,"fd0101",,"No Change"
HKR, Ndi\xparams\LED1PowerOn\enum,"40101",,"Slow blink"
HKR, Ndi\xparams\LED1PowerOn\enum,"30101",,"Regular blink"
HKR, Ndi\xparams\LED1PowerOn\enum,"20101",,"Fast blink"
HKR, Ndi\xparams\LED0PowerOff,ParamDesc,,"%LED0PowerOffStr%"
HKR, Ndi\xparams\LED0PowerOff,default,,"fe0001"
HKR, Ndi\xparams\LED0PowerOff,type,,enum
HKR, Ndi\xparams\LED0PowerOff\enum,"ff0001",,"LED Stays On"
HKR, Ndi\xparams\LED0PowerOff\enum,"fe0001",,"LED Stays Off"
HKR, Ndi\xparams\LED0PowerOff\enum,"fd0001",,"No Change"
HKR, Ndi\xparams\LED0PowerOff\enum,"40001",,"Slow blink"
HKR, Ndi\xparams\LED0PowerOff\enum,"30001",,"Regular blink"
HKR, Ndi\xparams\LED0PowerOff\enum,"20001",,"Fast blink"
HKR, Ndi\xparams\LED1PowerOff,ParamDesc,,"%LED1PowerOffStr%"
HKR, Ndi\xparams\LED1PowerOff,default,,"fe0101"
HKR, Ndi\xparams\LED1PowerOff,type,,enum
HKR, Ndi\xparams\LED1PowerOff\enum,"ff0101",,"LED Stays On"
HKR, Ndi\xparams\LED1PowerOff\enum,"fe0101",,"LED Stays Off"
HKR, Ndi\xparams\LED1PowerOff\enum,"fd0101",,"No Change"
HKR, Ndi\xparams\LED1PowerOff\enum,"40101",,"Slow blink"
HKR, Ndi\xparams\LED1PowerOff\enum,"30101",,"Regular blink"
HKR, Ndi\xparams\LED1PowerOff\enum,"20101",,"Fast blink"
HKR, Ndi\xparams\LED0Scan,ParamDesc,,"%LED0ScanStr%"
HKR, Ndi\xparams\LED0Scan,default,,"ff0001"
HKR, Ndi\xparams\LED0Scan,type,,enum
HKR, Ndi\xparams\LED0Scan\enum,"ff0001",,"LED Stays On"
HKR, Ndi\xparams\LED0Scan\enum,"fe0001",,"LED Stays Off"
HKR, Ndi\xparams\LED0Scan\enum,"fd0001",,"No Change"
HKR, Ndi\xparams\LED0Scan\enum,"40001",,"Slow blink"
HKR, Ndi\xparams\LED0Scan\enum,"30001",,"Regular blink"
HKR, Ndi\xparams\LED0Scan\enum,"20001",,"Fast blink"
HKR, Ndi\xparams\LED1Scan,ParamDesc,,"%LED1ScanStr%"
HKR, Ndi\xparams\LED1Scan,default,,"40101"
HKR, Ndi\xparams\LED1Scan,type,,enum
HKR, Ndi\xparams\LED1Scan\enum,"ff0101",,"LED Stays On"
HKR, Ndi\xparams\LED1Scan\enum,"fe0101",,"LED Stays Off"
HKR, Ndi\xparams\LED1Scan\enum,"fd0101",,"No Change"
HKR, Ndi\xparams\LED1Scan\enum,"40101",,"Slow blink"
HKR, Ndi\xparams\LED1Scan\enum,"30101",,"Regular blink"
HKR, Ndi\xparams\LED1Scan\enum,"20101",,"Fast blink"
HKR, Ndi\xparams\LED0Associated,ParamDesc,,"%LED0AssociatedStr%"
HKR, Ndi\xparams\LED0Associated,default,,"ff0001"
HKR, Ndi\xparams\LED0Associated,type,,enum
HKR, Ndi\xparams\LED0Associated\enum,"ff0001",,"LED Stays On"
HKR, Ndi\xparams\LED0Associated\enum,"fe0001",,"LED Stays Off"
HKR, Ndi\xparams\LED0Associated\enum,"fd0001",,"No Change"
HKR, Ndi\xparams\LED0Associated\enum,"40001",,"Slow blink"
HKR, Ndi\xparams\LED0Associated\enum,"30001",,"Regular blink"
HKR, Ndi\xparams\LED0Associated\enum,"20001",,"Fast blink"
HKR, Ndi\xparams\LED1Associated,ParamDesc,,"%LED1AssociatedStr%"
HKR, Ndi\xparams\LED1Associated,default,,"ff0101"
HKR, Ndi\xparams\LED1Associated,type,,enum
HKR, Ndi\xparams\LED1Associated\enum,"ff0101",,"LED Stays On"
HKR, Ndi\xparams\LED1Associated\enum,"fe0101",,"LED Stays Off"
HKR, Ndi\xparams\LED1Associated\enum,"fd0101",,"No Change"
HKR, Ndi\xparams\LED1Associated\enum,"40101",,"Slow blink"
HKR, Ndi\xparams\LED1Associated\enum,"30101",,"Regular blink"
HKR, Ndi\xparams\LED1Associated\enum,"20101",,"Fast blink"
HKR, Ndi\xparams\LED0Joined,ParamDesc,,"%LED0JoinedStr%"
HKR, Ndi\xparams\LED0Joined,default,,"ff0001"
HKR, Ndi\xparams\LED0Joined,type,,enum
HKR, Ndi\xparams\LED0Joined\enum,"ff0001",,"LED Stays On"
HKR, Ndi\xparams\LED0Joined\enum,"fe0001",,"LED Stays Off"
HKR, Ndi\xparams\LED0Joined\enum,"fd0001",,"No Change"
HKR, Ndi\xparams\LED0Joined\enum,"40001",,"Slow blink"
HKR, Ndi\xparams\LED0Joined\enum,"30001",,"Regular blink"
HKR, Ndi\xparams\LED0Joined\enum,"20001",,"Fast blink"
HKR, Ndi\xparams\LED1Joined,ParamDesc,,"%LED1JoinedStr%"
HKR, Ndi\xparams\LED1Joined,default,,"ff0101"
HKR, Ndi\xparams\LED1Joined,type,,enum
HKR, Ndi\xparams\LED1Joined\enum,"ff0101",,"LED Stays On"
HKR, Ndi\xparams\LED1Joined\enum,"fe0101",,"LED Stays Off"
HKR, Ndi\xparams\LED1Joined\enum,"fd0101",,"No Change"
HKR, Ndi\xparams\LED1Joined\enum,"40101",,"Slow blink"
HKR, Ndi\xparams\LED1Joined\enum,"30101",,"Regular blink"
HKR, Ndi\xparams\LED1Joined\enum,"20101",,"Fast blink"
HKR, Ndi\xparams\LED0Started,ParamDesc,,"%LED0StartedStr%"
HKR, Ndi\xparams\LED0Started,default,,"ff0001"
HKR, Ndi\xparams\LED0Started,type,,enum
HKR, Ndi\xparams\LED0Started\enum,"ff0001",,"LED Stays On"
HKR, Ndi\xparams\LED0Started\enum,"fe0001",,"LED Stays Off"
HKR, Ndi\xparams\LED0Started\enum,"fd0001",,"No Change"
HKR, Ndi\xparams\LED0Started\enum,"40001",,"Slow blink"
HKR, Ndi\xparams\LED0Started\enum,"30001",,"Regular blink"
HKR, Ndi\xparams\LED0Started\enum,"20001",,"Fast blink"
HKR, Ndi\xparams\LED1Started,ParamDesc,,"%LED1StartedStr%"
HKR, Ndi\xparams\LED1Started,default,,"ff0101"
HKR, Ndi\xparams\LED1Started,type,,enum
HKR, Ndi\xparams\LED1Started\enum,"ff0101",,"LED Stays On"
HKR, Ndi\xparams\LED1Started\enum,"fe0101",,"LED Stays Off"
HKR, Ndi\xparams\LED1Started\enum,"fd0101",,"No Change"
HKR, Ndi\xparams\LED1Started\enum,"40101",,"Slow blink"
HKR, Ndi\xparams\LED1Started\enum,"30101",,"Regular blink"
HKR, Ndi\xparams\LED1Started\enum,"20101",,"Fast blink"
HKR, Ndi\xparams\LED0Tx,ParamDesc,,"%LED0TxStr%"
HKR, Ndi\xparams\LED0Tx,default,,"ff0001"
HKR, Ndi\xparams\LED0Tx,type,,enum
HKR, Ndi\xparams\LED0Tx\enum,"ff0001",,"LED Stays On"
HKR, Ndi\xparams\LED0Tx\enum,"fe0001",,"LED Stays Off"
HKR, Ndi\xparams\LED0Tx\enum,"fd0001",,"No Change"
HKR, Ndi\xparams\LED0Tx\enum,"40001",,"Slow blink"
HKR, Ndi\xparams\LED0Tx\enum,"30001",,"Regular blink"
HKR, Ndi\xparams\LED0Tx\enum,"20001",,"Fast blink"
HKR, Ndi\xparams\LED1Tx,ParamDesc,,"%LED1TxStr%"
HKR, Ndi\xparams\LED1Tx,default,,"30101"
HKR, Ndi\xparams\LED1Tx,type,,enum
HKR, Ndi\xparams\LED1Tx\enum,"ff0101",,"LED Stays On"
HKR, Ndi\xparams\LED1Tx\enum,"fe0101",,"LED Stays Off"
HKR, Ndi\xparams\LED1Tx\enum,"fd0101",,"No Change"
HKR, Ndi\xparams\LED1Tx\enum,"40101",,"Slow blink"
HKR, Ndi\xparams\LED1Tx\enum,"30101",,"Regular blink"
HKR, Ndi\xparams\LED1Tx\enum,"20101",,"Fast blink"
HKR, Ndi\xparams\LED0Rx,ParamDesc,,"%LED0RxStr%"
HKR, Ndi\xparams\LED0Rx,default,,"ff0001"
HKR, Ndi\xparams\LED0Rx,type,,enum
HKR, Ndi\xparams\LED0Rx\enum,"ff0001",,"LED Stays On"
HKR, Ndi\xparams\LED0Rx\enum,"fe0001",,"LED Stays Off"
HKR, Ndi\xparams\LED0Rx\enum,"fd0001",,"No Change"
HKR, Ndi\xparams\LED0Rx\enum,"40001",,"Slow blink"
HKR, Ndi\xparams\LED0Rx\enum,"30001",,"Regular blink"
HKR, Ndi\xparams\LED0Rx\enum,"20001",,"Fast blink"
HKR, Ndi\xparams\LED1Rx,ParamDesc,,"%LED1RxStr%"
HKR, Ndi\xparams\LED1Rx,default,,"30101"
HKR, Ndi\xparams\LED1Rx,type,,enum
HKR, Ndi\xparams\LED1Rx\enum,"ff0101",,"LED Stays On"
HKR, Ndi\xparams\LED1Rx\enum,"fe0101",,"LED Stays Off"
HKR, Ndi\xparams\LED1Rx\enum,"fd0101",,"No Change"
HKR, Ndi\xparams\LED1Rx\enum,"40101",,"Slow blink"
HKR, Ndi\xparams\LED1Rx\enum,"30101",,"Regular blink"
HKR, Ndi\xparams\LED1Rx\enum,"20101",,"Fast blink"
HKR, Ndi\xparams\LED0TxHigh,ParamDesc,,"%LED0TxHighStr%"
HKR, Ndi\xparams\LED0TxHigh,default,,"ff0001"
HKR, Ndi\xparams\LED0TxHigh,type,,enum
HKR, Ndi\xparams\LED0TxHigh\enum,"ff0001",,"LED Stays On"
HKR, Ndi\xparams\LED0TxHigh\enum,"fe0001",,"LED Stays Off"
HKR, Ndi\xparams\LED0TxHigh\enum,"fd0001",,"No Change"
HKR, Ndi\xparams\LED0TxHigh\enum,"40001",,"Slow blink"
HKR, Ndi\xparams\LED0TxHigh\enum,"30001",,"Regular blink"
HKR, Ndi\xparams\LED0TxHigh\enum,"20001",,"Fast blink"
HKR, Ndi\xparams\LED1TxHigh,ParamDesc,,"%LED1TxHighStr%"
HKR, Ndi\xparams\LED1TxHigh,default,,"20101"
HKR, Ndi\xparams\LED1TxHigh,type,,enum
HKR, Ndi\xparams\LED1TxHigh\enum,"ff0101",,"LED Stays On"
HKR, Ndi\xparams\LED1TxHigh\enum,"fe0101",,"LED Stays Off"
HKR, Ndi\xparams\LED1TxHigh\enum,"fd0101",,"No Change"
HKR, Ndi\xparams\LED1TxHigh\enum,"40101",,"Slow blink"
HKR, Ndi\xparams\LED1TxHigh\enum,"30101",,"Regular blink"
HKR, Ndi\xparams\LED1TxHigh\enum,"20101",,"Fast blink"
HKR, Ndi\xparams\LED0RxHigh,ParamDesc,,"%LED0RxHighStr%"
HKR, Ndi\xparams\LED0RxHigh,default,,"ff0001"
HKR, Ndi\xparams\LED0RxHigh,type,,enum
HKR, Ndi\xparams\LED0RxHigh\enum,"ff0001",,"LED Stays On"
HKR, Ndi\xparams\LED0RxHigh\enum,"fe0001",,"LED Stays Off"
HKR, Ndi\xparams\LED0RxHigh\enum,"fd0001",,"No Change"
HKR, Ndi\xparams\LED0RxHigh\enum,"40001",,"Slow blink"
HKR, Ndi\xparams\LED0RxHigh\enum,"30001",,"Regular blink"
HKR, Ndi\xparams\LED0RxHigh\enum,"20001",,"Fast blink"
HKR, Ndi\xparams\LED1RxHigh,ParamDesc,,"%LED1RxHighStr%"
HKR, Ndi\xparams\LED1RxHigh,default,,"20101"
HKR, Ndi\xparams\LED1RxHigh,type,,enum
HKR, Ndi\xparams\LED1RxHigh\enum,"ff0101",,"LED Stays On"
HKR, Ndi\xparams\LED1RxHigh\enum,"fe0101",,"LED Stays Off"
HKR, Ndi\xparams\LED1RxHigh\enum,"fd0101",,"No Change"
HKR, Ndi\xparams\LED1RxHigh\enum,"40101",,"Slow blink"
HKR, Ndi\xparams\LED1RxHigh\enum,"30101",,"Regular blink"
HKR, Ndi\xparams\LED1RxHigh\enum,"20101",,"Fast blink"
HKR,, LEDOffAfterRadioOff, 2, "1"
HKR, Ndi\xparams\DataRate,ParamDesc,,"%DataRate%"
HKR, Ndi\xparams\DataRate,default,,"FF"
HKR, Ndi\xparams\DataRate,type,,enum
HKR, Ndi\xparams\DataRate\enum,"FF",,"Auto"
HKR, Ndi\xparams\DataRate\enum,"2",,"1 Mbps"
HKR, Ndi\xparams\DataRate\enum,"4",,"2 Mbps"
HKR, Ndi\xparams\DataRate\enum,"b",,"5.5 Mbps"
HKR, Ndi\xparams\DataRate\enum,"16",,"11 Mbps"
HKR, Ndi\xparams\DataRate\enum,"C",,"6 Mbps"
HKR, Ndi\xparams\DataRate\enum,"12",,"9 Mbps"
HKR, Ndi\xparams\DataRate\enum,"18",,"12 Mbps"
HKR, Ndi\xparams\DataRate\enum,"24",,"18 Mbps"
HKR, Ndi\xparams\DataRate\enum,"30",,"24 Mbps"
HKR, Ndi\xparams\DataRate\enum,"48",,"36 Mbps"
HKR, Ndi\xparams\DataRate\enum,"60",,"48 Mbps"
HKR, Ndi\xparams\DataRate\enum,"6C",,"54 Mbps"
HKR, Ndi\xparams\WepStatus,ParamDesc,,"%WepStatus%"
HKR, Ndi\xparams\WepStatus,default,,"1"
HKR, Ndi\xparams\WepStatus,type,,enum
HKR, Ndi\xparams\WepStatus\enum,"0",,"Enabled"
HKR, Ndi\xparams\WepStatus\enum,"1",,"Disabled"
HKR,, TxWepKey, 2, ""
HKR,, WepKey1, 2, ""
HKR,, WepKey2, 2, ""
HKR,, WepKey3, 2, ""
HKR,, WepKey4, 2, ""
HKR,, WIFI, 2, "0"
HKR,, DriverRel, 2, "12/30/2005"
[W8335PCIXP.zerocfg]
[Strings]
MRVL="Marvell"
TxAntennaStr="Tx Antenna Select"
RxAntennaStr="Rx Antenna Select"
Channel="Channel"
FragThsd="Fragamentation Threshold"
DataRate="Data Rate"
RTSThsd="RTS Threshold"
AuthMode="Authentication Mode"
NetworkMode="Operation Mode"
WepStatus="WEP Status"
SSID="SSID"
PreambleStr="Preamble Select"
PowerMode="Power Save Mode"
AdhocGMode="Adhoc Mode"
WMM="WMM"
WIFI="WIFI"
LED0PowerOnStr="LED 0 Power On"
LED0PowerOffStr="LED 0 Power Off"
LED0ScanStr="LED 0 Site Survey"
LED0AssociatedStr="LED 0 Associated"
LED0JoinedStr="LED 0 IBSS Joined"
LED0StartedStr="LED 0 IBSS Started"
LED0TxStr="LED 0 Tx"
LED0RxStr="LED 0 Rx"
LED0TxHighStr="LED 0 Tx High Traffic"
LED0RxHighStr="LED 0 Rx High Traffic"
LED1PowerOnStr="LED 1 Power On"
LED1PowerOffStr="LED 1 Power Off"
LED1ScanStr="LED 1 Site Survey"
LED1AssociatedStr="LED 1 Associated"
LED1JoinedStr="LED 1 IBSS Joined"
LED1StartedStr="LED 1 IBSS Started"
LED1TxStr="LED 1 Tx"
LED1RxStr="LED 1 Rx"
LED1TxHighStr="LED 1 Tx High Traffic"
LED1RxHighStr="LED 1 Rx High Traffic"
RegionControl="Region Control"
W8335PCI.DeviceDesc="802.11g/b Wireless LAN Client Adapter"
W8335PXPCI.DeviceDesc="802.11g/b Wireless LAN Client Adapter"
W8335PCIXP.Service.DispName="802.11g/b Driver for Windows XP (8335)"
W8335PCI2K.Service.DispName="802.11g/b Driver for Windows 2K (8335)"

