
[Version]
DriverVer=06/03/2004, 3.0.18.2
Signature="$Chicago$"
Compatible=1
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%DRV_PROVIDER_STR%
CatalogFile.NT=WlanUIG.cat
[ControlFlags]
ExcludeFromSelect=*
[Manufacturer]
%MANUFACTURER_STR%=DeviceList, NT.5.1
[DeviceList.NT.5.1] ; WinXP
%WLAN_USB_DESC_STR%=WLAN_USB1.NT.5.1, USB\VID_0CDE&PID_0008 ;XG703
%WLAN_USB_DESC_STR%=WLAN_USB2.NT.5.1, USB\Vid_0cde&Pid_0006 ;XG702
[DeviceList]
%WLAN_USB_DESC_STR%=WLAN_USB1, USB\VID_0CDE&PID_0008
%WLAN_USB_DESC_STR%=WLAN_USB2, USB\Vid_0cde&Pid_0006
[WLAN_USB1.NT.5.1] ; WinXP
AddReg=WLAN_USB1_XP_REG, COMMON_USB_REG, COMMON_NDIS_REG_NT, COMMON_REG
;CpyFiles=WLAN_USB_DRIVER_COPY_NT
BusType=15 ;USB
Characteristics= 0x84
[WLAN_USB1.NT.5.1.Services]
AddService= "WlanUIG", 2, WLAN_DRIVER_USB_SERVICE, WLAN_USB_DRIVER_EVENTLOG
[WLAN_USB1_XP_REG]
HKR,Ndi,DeviceID,0,"USB\VID_0CDE&PID_0008"
HKR,,PlatformID,0,14480
HKR,,UsbVariant,0,14471
HKR,,VendorDesc,0,%WLAN_USB_DESC_STR%
[WLAN_USB1.NT] ; Win2k
AddReg=WLAN_USB1_2K_REG, COMMON_USB_REG, COMMON_NDIS_REG_NT, COMMON_REG
;CpyFiles=WLAN_USB_DRIVER_COPY_NT
BusType=15 ;USB
Characteristics= 0x84
[WLAN_USB1.NT.Services]
AddService= "WlanUIG", 2, WLAN_DRIVER_USB_SERVICE, WLAN_USB_DRIVER_EVENTLOG
[WLAN_USB1_2K_REG]
HKR,Ndi,DeviceID,0,"USB\VID_0CDE&PID_0008"
HKR,,PlatformID,0,14480
HKR,,UsbVariant,0,14471
HKR,,VendorDesc,0,%WLAN_USB_DESC_STR%
[WLAN_USB1] ; Win9x
AddReg=WLAN_USB1_REG, COMMON_USB_REG, COMMON_NDIS_REG_9x, COMMON_REG
;CpyFiles=WLAN_USB_DRIVER_COPY
[WLAN_USB1_REG]
HKR,Ndi,DeviceID,0,"USB\VID_0CDE&PID_0008"
HKR,,PlatformID,0,14480
HKR,,UsbVariant,0,14471
HKR,,VendorDesc,0,%WLAN_USB_DESC_STR%
[WLAN_USB2.NT.5.1] ; WinXP
AddReg=WLAN_USB2_XP_REG, COMMON_USB_REG, COMMON_NDIS_REG_NT, COMMON_REG
;CpyFiles=WLAN_USB_DRIVER_COPY_NT
BusType=15 ;USB
Characteristics= 0x84
[WLAN_USB2.NT.5.1.Services]
AddService= "WlanUIG", 2, WLAN_DRIVER_USB_SERVICE, WLAN_USB_DRIVER_EVENTLOG
[WLAN_USB2_XP_REG]
HKR,Ndi,DeviceID,0,"USB\Vid_0cde&Pid_0006"
HKR,,PlatformID,0,14480
HKR,,UsbVariant,0,8832
HKR,,VendorDesc,0,%WLAN_USB_DESC_STR%
[WLAN_USB2.NT] ; Win2k
AddReg=WLAN_USB2_2K_REG, COMMON_USB_REG, COMMON_NDIS_REG_NT, COMMON_REG
;CpyFiles=WLAN_USB_DRIVER_COPY_NT
BusType=15 ;USB
Characteristics= 0x84
[WLAN_USB2.NT.Services]
AddService= "WlanUIG", 2, WLAN_DRIVER_USB_SERVICE, WLAN_USB_DRIVER_EVENTLOG
[WLAN_USB2_2K_REG]
HKR,Ndi,DeviceID,0,"USB\Vid_0cde&Pid_0006"
HKR,,PlatformID,0,14480
HKR,,UsbVariant,0,8832
HKR,,VendorDesc,0,%WLAN_USB_DESC_STR%
[WLAN_USB2] ; Win9x
AddReg=WLAN_USB2_REG, COMMON_USB_REG, COMMON_NDIS_REG_9x, COMMON_REG
;CpyFiles=WLAN_USB_DRIVER_COPY
[WLAN_USB2_REG]
HKR,Ndi,DeviceID,0,"USB\Vid_0cde&Pid_0006"
HKR,,PlatformID,0,14480
HKR,,UsbVariant,0,8832
HKR,,VendorDesc,0,%WLAN_USB_DESC_STR%
[WLAN_DRIVER_USB_SERVICE] ;Win2k
DisplayName=%WLAN_USB_SERVICE_STR%
ServiceType=1 ; SERVICE_KERNEL_DRIVER
StartType=3 ; SERVICE_DEMAND_START
ErrorControl=1 ; NORMAL
ServiceBinary=%12%\WlanUIG.sys
LoadOrderGroup=NDIS
[WLAN_USB_DRIVER_EVENTLOG]
AddReg=WLAN_USB_DRIVER_EVENTLOG_REG
[WLAN_USB_DRIVER_EVENTLOG_REG]
HKR, ,EventMessageFile ,0x00020000 ,"%%SystemRoot%%\System32\netevent.dll"
HKR, ,TypesSupported ,0x00010001 ,7
[COMMON_NDIS_REG_NT]
HKR,NDI\Interfaces ,UpperRange ,0 ,"ndis5"
HKR,NDI\Interfaces ,LowerRange ,0 ,"ethernet"
HKR,NDI ,Service ,0 ,"WlanUIG"
HKR, ,DeviceVxDs ,0 ,"WlanUIG.sys"
[COMMON_NDIS_REG_9x]
HKR, ,RunningWin9X ,0 ,"1"
HKR, ,DevLoader ,0 ,"*ndis"
HKR, ,EnumPropPages ,0 ,"netdi.dll,EnumPropPages"
HKR,NDI\Interfaces ,UpperRange ,0 ,"ndis3"
HKR,NDI\Interfaces ,LowerRange ,0 ,"ethernet"
HKR,NDI\Interfaces ,DefUpper ,0 ,"ndis3"
HKR,NDI\Interfaces ,DefLower ,0 ,"ethernet"
HKR,NDIS ,LogDriverName ,0 ,"WLANUI9X"
HKR,NDIS ,MajorNdisVersion ,1 ,04
HKR,NDIS ,MinorNdisVersion ,1 ,00
HKR,NDI ,Service ,0 ,"WlanUI9X"
HKR, ,DeviceVxDs ,0 ,"WlanUI9X.sys"
[COMMON_USB_REG]
HKR,NDI ,CardType ,0 ,"USB"
HKR, ,BusType ,0 ,"0" ; Inconsistency with earlier definition is needed.
[COMMON_REG]
HKR, ,WLANIOC ,0 ,"XG-300"
HKR, ,RTSThresh ,0 ,2347
HKR,defaults ,RTSThresh ,0 ,2347
HKR, ,FragThresh ,0 ,2346
HKR,defaults ,FragThresh ,0 ,2346
HKR, ,ConfigProfile ,0 ,256
HKR,defaults ,ConfigProfile ,0 ,256
HKR, ,NitroMode ,0 ,1
HKR,defaults ,NitroMode ,0 ,1
HKR, ,PSMode ,0 ,1
HKR,defaults ,PSMode ,0 ,1
HKR, ,SSID ,0 ,"ANY"
HKR,defaults ,SSID ,0 ,"ANY" ;Default value is "any"
HKR, ,NetworkType ,0 ,1
HKR,defaults ,NetworkType ,0 ,1 ;Infrasturcture
HKR,Ndi\params\PSMode,default,0,1
HKR,NDI\params\PSMode,ParamDesc,0,%POWER_SAVE_STR%
HKR,NDI\params\PSMode,type,0,"enum"
HKR,NDI\params\PSMode,flag,1,30,00,00,00
HKR,NDI\params\PSMode\enum,1,,%POWER_SAVE_OFF_STR%
HKR,NDI\params\PSMode\enum,2,,%POWER_SAVE_DYN_STR%
HKR,NDI\params\PSMode\enum,3,,%POWER_SAVE_MAX_STR%
HKR,NDI\params\ConfigProfile,default,0,256
HKR,NDI\params\ConfigProfile,ParamDesc,,%CONFIG_PROFILE%
HKR,NDI\params\ConfigProfile,type,0,"enum"
HKR,NDI\params\ConfigProfile,flag,1,30,00,00,00
HKR,NDI\params\ConfigProfile\enum,0,,%CONFIG_PROF_B_ONLY%
HKR,NDI\params\ConfigProfile\enum,1,,%CONFIG_PROF_MIXED%
HKR,NDI\params\ConfigProfile\enum,2,,%CONFIG_PROF_MIXED_LONG%
HKR,NDI\params\ConfigProfile\enum,3,,%CONFIG_PROF_G_ONLY%
HKR,NDI\params\ConfigProfile\enum,4,,%CONFIG_PROF_TEST%
HKR,NDI\params\ConfigProfile\enum,5,,%CONFIG_PROF_B_WIFI%
HKR,NDI\params\ConfigProfile\enum,6,,%CONFIG_PROF_MIXED_SHORT%
HKR,NDI\params\ConfigProfile\enum,256,,%CONFIG_PROF_WIFI_SPEC%
HKR,NDI\params\NitroMode,default,0,1
HKR,NDI\params\NitroMode,ParamDesc,,%NITRO_MODE%
HKR,NDI\params\NitroMode,type,,enum
HKR,NDI\params\NitroMode,flag,1,30,00,00,00
HKR,NDI\params\NitroMode\enum,0,,%OFF_STR%
HKR,NDI\params\NitroMode\enum,1,,%ON_STR%
HKR,Ndi\params\RTSThresh,default,0,2347
HKR,NDI\params\RTSThresh,ParamDesc,0,%RTSTHRESH_STR%
HKR,NDI\params\RTSThresh,type,0,int
HKR,NDI\params\RTSThresh,flag,1,20,00,00,00
HKR,NDI\params\RTSThresh,min,0,0
HKR,NDI\params\RTSThresh,max,0,2347
HKR,NDI\params\RTSThresh,step,0,1
HKR,Ndi\params\FragThresh,default,0,2346
HKR,NDI\params\FragThresh,ParamDesc,0,%FRAGTHRESH_STR%
HKR,NDI\params\FragThresh,type,0,int
HKR,NDI\params\FragThresh,flag,1,20,00,00,00
HKR,NDI\params\FragThresh,min,0,256
HKR,NDI\params\FragThresh,max,0,2346
HKR,NDI\params\FragThresh,step,0,2
HKR,NDI\params\PpePdlpEnable,default,0,0
HKR,NDI\params\PpePdlpEnable,ParamDesc,,%PPE_PDLP%
HKR,NDI\params\PpePdlpEnable,type,,enum
HKR,NDI\params\PpePdlpEnable,flag,1,30,00,00,00
HKR,NDI\params\PpePdlpEnable\enum,0,,%OFF_STR%
HKR,NDI\params\PpePdlpEnable\enum,1,,%ON_STR%
HKR,NDI\params\PpeCompressEnable,default,0,0
HKR,NDI\params\PpeCompressEnable,ParamDesc,,%PPE_COMPRESS%
HKR,NDI\params\PpeCompressEnable,type,,enum
HKR,NDI\params\PpeCompressEnable,flag,1,30,00,00,00
HKR,NDI\params\PpeCompressEnable\enum,0,,%OFF_STR%
HKR,NDI\params\PpeCompressEnable\enum,1,,%ON_STR%
HKR,NDI\params\PpeConcatEnable,default,0,0
HKR,NDI\params\PpeConcatEnable,ParamDesc,,%PPE_CONCAT%
HKR,NDI\params\PpeConcatEnable,type,,enum
HKR,NDI\params\PpeConcatEnable,flag,1,30,00,00,00
HKR,NDI\params\PpeConcatEnable\enum,0,,%OFF_STR%
HKR,NDI\params\PpeConcatEnable\enum,1,,%ON_STR%
HKR,NDI\params\PpePiggyBackEnable,default,0,0
HKR,NDI\params\PpePiggyBackEnable,ParamDesc,,%PPE_PIGGYBACK%
HKR,NDI\params\PpePiggyBackEnable,type,,enum
HKR,NDI\params\PpePiggyBackEnable,flag,1,30,00,00,00
HKR,NDI\params\PpePiggyBackEnable\enum,0,,%OFF_STR%
HKR,NDI\params\PpePiggyBackEnable\enum,1,,%ON_STR%
HKR, Ndi\params\11dMode,default,0,2
HKR, Ndi\params\11dMode,ParamDesc,0,%11D_MODE%
HKR, Ndi\params\11dMode,type,0 ,"enum"
HKR, Ndi\params\11dMode\enum,0 ,0,"Disabled"
HKR, Ndi\params\11dMode\enum,1 ,0,"Strict"
HKR, Ndi\params\11dMode\enum,2 ,0,"Flexible"
[DestinationDirs]
WLAN_USB_DRIVER_COPY_NT=12 ; Win2k=%windir%\system32\drivers
WLAN_USB_DRIVER_COPY=11 ; Win9x=%windir%\system
[WLAN_USB_DRIVER_COPY_NT]
WlanUIG.sys
[WLAN_USB_DRIVER_COPY]
WlanUI9X.sys
[SourceDisksNames]
1=%INSTALL_DISK_STR%,,,
[SourceDisksFiles] ; Win9x
WlanUIG.sys=1
WlanUI9X.sys=1
[Strings]
DRV_PROVIDER_STR=" "
MANUFACTURER_STR=" "
WLAN_USB_SERVICE_STR="NB 802.11g Wireless LAN USB Adapter Driver"
INSTALL_DISK_STR="NB 802.11g Wireless LAN USB Adapter Install Disk"
WLAN_USB_DESC_STR="NB 802.11g Wireless LAN USB Adapter"
POWER_SAVE_STR="Power Save Mode"
POWER_SAVE_OFF_STR="Disabled"
POWER_SAVE_DYN_STR="Dynamic"
POWER_SAVE_MAX_STR="Maximum"
RTSTHRESH_STR="RTS Threshold"
FRAGTHRESH_STR="Fragmentation Threshold"
ON_STR="On"
OFF_STR="Off"
CONFIG_PROFILE="Configuration Profile"
CONFIG_PROF_B_ONLY="B only"
CONFIG_PROF_MIXED="Mixed"
CONFIG_PROF_MIXED_LONG="Mixed Long"
CONFIG_PROF_G_ONLY="G only"
CONFIG_PROF_TEST="Test"
CONFIG_PROF_B_WIFI="B WiFi"
CONFIG_PROF_MIXED_SHORT="Mixed Short"
CONFIG_PROF_WIFI_SPEC="WiFi Spec"
NITRO_MODE="Nitro Mode"
PPE_PDLP="Direct Link"
PPE_COMPRESS="Compression"
PPE_CONCAT="Concatenation"
PPE_PIGGYBACK="PiggyBack"
11D_MODE="11D Mode"
